CONFUSION PULL UP PULL DOWN

button with PULL\_DOWN - connect the other pin to VCC

PULL\_DOWN button status Should be 0 when not pressed, 1 when pressed

button with PULL\_UP - connect the other pin to GND

PULL\_UP Should be 1 when not pressed, 0 when pressed

PULL\_UP Should be 1 when not pressed, 0 when pressed